##### **PRESS RELEASE**

FOR IMMEDIATE RELEASE:

February 2, 2026

(*Please do not publish beyond 6 months from this date*)

Contact: Libby Beck

Phone: 608-897-2131, Ext. 2271

[libby.beck@kuhn.com](mailto:libby.beck@kuhn.com)

**New KUHN Knight SLC 200 Series ProTwin® Slinger® Commercial Manure Spreaders**

KUHN North America proudly introduces the new KUHN Knight SLC 200 Series ProTwin® Slinger® commercial manure spreaders, continuing the trusted legacy of rugged construction, superior material breakup, and reliable performance in the toughest conditions.

Engineered to handle heavy, sand-laden manure and the widest variety of materials, the SLC 200 Series builds on KUHN’s proven ProTwin Slinger technology for unmatched versatility and durability. Available in both truck-mount and trailer configurations, these spreaders offer capacities from 3,200 to 5,000 gallons to fit a range of operations. They deliver fast unloading and superior material breakup—ensuring consistent, even spreading and maximum productivity. Exclusive V-body construction eliminates bridging for smooth material flow, while the wide 18-hammer discharge improves material breakup and speeds up unloading. A fully enclosed, heavy-duty drive system reduces maintenance and extends component life, and independent auger protection safeguards critical components against overloads and obstructions.

KUHN Knight SLC 200 Series ProTwin® Slinger® commercial manure spreaders are now available through authorized KUHN dealers across North America. To locate a dealer or learn more about the SLC 200 series visit our website: [www.kuhn.com](http://www.kuhn.com).

Kuhn North America, Inc., of Brodhead, Wisconsin, is a leading innovator in agricultural and industrial equipment. KUHN offers a broad range of hay and forage, livestock and crop production tools, as well as landscape and road maintenance equipment. KUHN, KUHN Knight and KUHN Krause products are sold by farm equipment dealers throughout the United States, Canada and many other countries.